,WIDTH##OTHER##,WEIGHT##OTHER##,URL##OTHER##,UPHOLSTERY MATERIAL EXTERIOR##OTHER##,UPHOLSTERY MATERIAL##OTHER##,TECHNICAL SHEET##OTHER##,PRODUCT SHEET##OTHER##,PRODUCT CODE##OTHER##,Modelo##OTHER##,Fabricante##OTHER##,MATERIAL DESCRIPTION##OTHER##,HEIGHT##OTHER##,Descripción##OTHER##,DEPTH##OTHER##,BIM USER MANUAL##OTHER##,BIM AUTHOR##OTHER##,BADGE##OTHER##
ARMCHAIR  347.11.N,108 cm,36.0 kg,https://sancal.com/en/,UPHOLSTERY_MATERIAL_6115,UPHOLSTERY_MATERIAL_6118,https://sancal.com/en/,https://www.archiproducts.com/en/sancal,347.11.N,REMNANT,Sancal,Upholstered fabric quilted with fibre. Back-arm structure: injection moulded foam over an F1 steel frame with an MDF base. Seat structure: injection moulded foam over an F1 steel sprung frame covered in 100g fibre. Height adjustable stoppers.,73 cm,Upholstered fabric armchair by Note Design Studio.,85 cm,https://img.edilportale.com/bim/SANCAL-BIM-USER-MANUAL-SANCAL-bim.pdf,https://sancal.com/,https://bim.archiproducts.com/en/badge/bim-archiproducts-featured_658700/about
